:Base PDR21PD
1 [Setup] Tab
2 Orientation=VDS_IDH_01_SETUP_ORIENTATION
2 Number of copies=VDS_IDH_01_SETUP_COPIES
2 Turns over the card after loading=VDS_IDH_01_SETUP_TURN_CARD_LOAD
2 Load ...=VDS_IDH_01_SETUP_PROFILE_LOAD
2 Save ...=VDS_IDH_01_SETUP_PROFILE_SAVE
1 [Print] Tab
2 Print=VDS_IDH_02_PRNT_SINGLE
2 Print on both sides=VDS_IDH_02_PRNT_BOTH
2 Print the back side first=VDS_IDH_02_PRNT_BACK_FIRST
2 Print mode=VDS_IDH_02_PRNT_MODE
2 Using of Resin K ink=VDS_IDH_02_PRNT_K_EXT
2 Security erase=VDS_IDH_02_PRNT_K_SEC
2 Rotate by 180=VDS_IDH_02_PRNT_ROTATE
2 Enable the printing area=VDS_IDH_02_PRNT_AREA
2 Enable the color adjustment=VDS_IDH_02_PRNT_COLOR
2 Enable the look-up table=VDS_IDH_02_PRNT_LUT
2 Dither ...=VDS_IDH_02_PRNT_DITHER
2 UV ink ...=VDS_IDH_02_PRNT_SP1
2 Enable the printer settings=VDS_IDH_02_PRNT_SETTING
2 [Printing area] Dialog
3 Rectangular region list=VDS_IDH_11_AREA_LIST
3 X=VDS_IDH_11_AREA_X
3 Y=VDS_IDH_11_AREA_Y
3 W=VDS_IDH_11_AREA_DX
3 H=VDS_IDH_11_AREA_DY
3 Ink=VDS_IDH_11_AREA_PLANE
3 Side=VDS_IDH_11_AREA_SIDE
3 Add=VDS_IDH_11_AREA_ADD
3 Delete=VDS_IDH_11_AREA_DEL
3 Delete All=VDS_IDH_11_AREA_CLEAR
3 Peeloff ink energy=VDS_IDH_11_AREA_ENERGY
2 [Color] Dialog
3 Brightness=VDS_IDH_12_COLOR_BRIGHTNESS
3 Contrast=VDS_IDH_12_COLOR_CONTRAST
3 Hue=VDS_IDH_12_COLOR_HUE
3 Gamma=VDS_IDH_12_COLOR_GAMMA
3 Default=VDS_IDH_12_COLOR_DEFAULT
2 [Look up table] Dialog
3 Look up table list=VDS_IDH_13_LUT_LIST
3 Name=VDS_IDH_13_LUT_NAME
3 File=VDS_IDH_13_LUT_FILE
3 Add=VDS_IDH_13_LUT_ADD
3 Delete=VDS_IDH_13_LUT_DEL
3 Delete All=VDS_IDH_13_LUT_CLEAR
2 [Dither] Dialog
3 Image adjustment=VDS_IDH_14_DITHER_GAMMA
3 Default=VDS_IDH_14_DITHER_DEFAULT
2 [UV ink] Dialog
3 Extraction=VDS_IDH_15_SP1_EXT
4 Text=VDS_IDH_15_SP1_EXT_TXT
4 File=VDS_IDH_15_SP1_EXT_FILE
3 Page split=VDS_IDH_15_SP1_PAGE
3 No printing color=VDS_IDH_15_SP1_BACKCOLOR
3 MAC address position=VDS_IDH_15_SP1_MAC_POSITION
3 File information=VDS_IDH_15_SP1_FILE_LIST
4 Name=VDS_IDH_15_SP1_FILE_NAME
4 File=VDS_IDH_15_SP1_FILE_PATH
4 X=VDS_IDH_15_SP1_FILE_X
4 Y=VDS_IDH_15_SP1_FILE_Y
4 Side=VDS_IDH_15_SP1_FILE_SIDE
4 Add=VDS_IDH_15_SP1_FILE_ADD
4 Delete=VDS_IDH_15_SP1_FILE_DEL
4 Delete All=VDS_IDH_15_SP1_FILE_CLEAR
3 Number of panels using the retransfer film=VDS_IDH_15_SP1_PANEL
2 [Printer settings] Dialog
3 YMC ink print level=VDS_IDH_16_SET_YMC_LV
3 Resin K ink print level=VDS_IDH_16_SET_K_LV
3 UV ink print level=VDS_IDH_16_SET_SP1_LV
3 Peeloff ink print level=VDS_IDH_16_SET_SP2_LV
3 Resin K ink print mode=VDS_IDH_16_SET_K_MODE
3 MG Peel mode=VDS_IDH_16_SET_MG_PRINT
3 Standby mode=VDS_IDH_16_SET_RT_STANDBY
3 Back side cooling=VDS_IDH_16_SET_BACK_COOL
3 Retransfer=VDS_IDH_16_SET_RETRANSFER
3 UV speed=VDS_IDH_16_SET_UV_SPEED
3 Bend remedy=VDS_IDH_16_SET_CARD
1 [Encode] Tab
2 Non-contact IC encode=VDS_IDH_03_ENCD_IC_CONLESS
2 Contact IC encode=VDS_IDH_03_ENCD_IC_CONTACT
2 Turns over the card after IC encoding=VDS_IDH_03_ENCD_IC_TURN
2 Magnetic encode=VDS_IDH_03_ENCD_MG
2 Turns over the card after MG encoding=VDS_IDH_03_ENCD_MG_TURN
2 Write retry=VDS_IDH_03_ENCD_MG_RETRY
2 Coercivity=VDS_IDH_03_ENCD_MG_COERCIVITY
2 Inline type=VDS_IDH_03_ENCD_MG_INLINE
2 Starts from magnetic encoding=VDS_IDH_03_ENCD_SEQUENCE
2 Prints after encoding=VDS_IDH_03_ENCD_WAIT
1 [Laminate] Tab
2 Mode=VDS_IDH_04_LMNT_MODE
1 [Configuration] Tab
2 Turnover unit=VDS_IDH_05_UNIT_TURNOVER
2 Bend remedy unit=VDS_IDH_05_UNIT_REMEDY
2 Non-contact IC encoder=VDS_IDH_05_UNIT_CONLESS
2 ISO Contact IC encoder=VDS_IDH_05_UNIT_IC_ISO
2 JIS Contact IC encoder=VDS_IDH_05_UNIT_IC_JIS
2 ISO Magnetic encoder=VDS_IDH_05_UNIT_MG_ISO
2 JIS Magnetic encoder=VDS_IDH_05_UNIT_MG_JIS
2 Laminator=VDS_IDH_05_UNIT_LAMINATE
2 Enable the settings=VDS_IDH_05_UNIT_SETTING
1 [Version] Tab
