This demo commission first formats a DESFire transponder and then adds an application with two files. If the PICC Master Key is not set to the factory setting of 0x00 00 00 00 00 00 00 00 (DES), the coding will fail.

Created Applications/Files:

1) AID F3ADA0
   Key Settings: 0x1B
   Key Type: AES
   Number of keys: 4
   Key 0: 0x00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
   Key 1: 0x11 11 11 11 11 11 11 11 11 11 11 11 11 11 11 11
   Key 2: 0x22 22 22 22 22 22 22 22 22 22 22 22 22 22 22 22
   Key 3: 0x33 33 33 33 33 33 33 33 33 33 33 33 33 33 33 33
   
   1a) File 0
       Data: Byte 0 - 2.5: Card ID, BCD (20 bit)
             Byte 2.5 - 4: Card ID, HEX (20 bit)
		     Byte 5 - 9: Card ID, ASCII (40 bit)
             Byte 10: Inverted XOR CRC over Byte 0-9 (8 bit)
	   Access Rights: 0x2331 (Read Key 2, Write Key 3, Read/Write Key 3, Change Access Rights Key 1)
	   
   1b) File 1
       Data: Byte 0 - 15: Card ID, ASCII (128 bit)
             Byte 16 - 44: Fix data "© MADA Marx Datentechnik GmbH", ASCII (232 bit)   
	   Access Rights: 0xE331 (Read Key Free Access, Write Key 3, Read/Write Key 3, Change Access Rights Key 1)

The corresponding .RDX file allows reading the coded card ID.